GP maintenance window:

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Window Name** | **Execution Time** | **Outage Time** | **Critical** | **Major** | **Minor** | **Info** | **Remarks** |
| Window-1 | 00:00 - 06:00 | 02:00 - 05:00 | Yes | Yes | Yes | Yes | All types of Planned Work/Maintenance activities which may lead outage or may have high risk. |
| Window-2 | 06:00 - 09:00 | 06:00 - 09:00 | No | No | Yes | Yes | Maximum 15 sites |
| Window-3 | 13:00 - 17:00 | 13:00 - 17:00 | No | No | Yes | Yes | Maximum 5 sites |
| Window-4 (data) | 03:00 - 07:00 | 03:00 - 07:00 | Yes | Yes | Yes | Yes | Data Affected Planned Activity |
| Window-5 | 10:00 - 17:00 | 10:00 - 17:00 <30 Mins outage of One Site | No | No | Yes | Yes | Single Site Outage Duration <30 mins |
| Info CR | No | No | No | Yes | Information RFC |